{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["Info","Reinforcement","Foundation","Soil","Loading","Settings","DesignSettings","Enums"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":21,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Info","index":0,"n_rows":8,"n_cols":2,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Field","Value"]
["Project","SkyVim"]
["Name","Fnd 010"]
["Description"]
["Location","Florence"]
["Company","StruSoft"]
["Signature","MP"]
["Comments","Optimal Foundation"]

{"sheet":"Reinforcement","index":1,"n_rows":5,"n_cols":6,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["Direction","Diameter","Spacing","Cover","Zone","Material"]
["X",12,200,35,"TOP","B500"]
["X",12,200,35,"BOTTOM","B500"]
["Y",12,200,35,"TOP","B500"]
["Y",12,200,35,"BOTTOM","B500"]

{"sheet":"Foundation","index":2,"n_rows":13,"n_cols":3,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Field","Value","Units"]
["Type","Point","-"]
["Lx bottom",1.4,"[m]"]
["Ly bottom",2,"[m]"]
["Lx top",0.3,"[m]"]
["Ly top",0.3,"[m]"]
["Height",0.5,"[m]"]
["Eccentricity x",0.1,"[m]"]
["Eccentricity y",0.15,"[m]"]
["Material","C30/37","-"]
["Top of footing",-0.1,"[m]"]
["Position x",0,"[m]"]
["Position y",0,"[m]"]

{"sheet":"Soil","index":3,"n_rows":13,"n_cols":14,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["INPUT MODE","Simple"]
[]
["SIMPLE SOIL"]
["Field","Value","Units"]
["Allowed soil pressure SLS",100,"kN/mq"]
["Allowed soil pressure ULS",150,"kN/mq"]
["Friction coefficient",0.25,"-"]
[]
[]
[]
["COMPLEX SOIL"]
["Name","Type","phik","ck","cuk","rk","gamma","gamma eff","m0","Top of Layer [m]",null,null,"Depth limit [m]",-10]
["Silty Clay","Drained",30,10,"-","-",18,10,20000,0,null,null,"Ground water [m]",-1.2]

{"sheet":"Loading","index":4,"n_rows":4,"n_cols":8,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["Name","Type","Hx [kN]","Hy [kN]","N [kN]","Mx [kNm]","My [kNm]","SW [-]"]
["Combo 1","CHARACTERISTIC",0,0,300,2,1,1]
["Combo 2","FREQUENT",0,23,0,3,2,1]
["Combo 3","ULTIMATE",10,0,0,1,3,1]

{"sheet":"Settings","index":5,"n_rows":22,"n_cols":2,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["CODE SETTINGS"]
["Annex","ANNEX_SWEDEN"]
["Consequence","CONSEQUENCE_CLASS_2"]
["Reliability","RELIABILITY_CLASS_2"]
[]
["CONCRETE SETTINGS"]
["Crack",0.01]
["Distribution","FOUNDATION_DISTRIBUTION_PLASTIC"]
["Fabrication","FABRICATION_PREFAB"]
["Low strength variation",true]
["Consider min reinforcement",true]
["Exposure class","EXPOSURE_CLASS_XC1"]
["Life category","LIFE_CATEGORY_L50"]
["Critical element",false]
["Inspection level","INSPECTION_LEVEL_NORMAL"]
[]
["SOIL SETTINGS"]
["Des approach","DESIGN_APPROACH_2"]
["Geo category","GEOTECHNICAL_CATEGORY_1"]
["Check settlement",true]
["Absolute settlement",20]
["Punching","SOIL_PUNCHING_TYPE_1_2"]

{"sheet":"DesignSettings","index":6,"n_rows":13,"n_cols":8,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Steel design settings"]
["REINF DIAMETERS [mm]","SPACING MIN [mm]","SPACING MAX [mm]","STEP [mm]"]
["8, 10, 12",100,200,25]
[]
[]
["Concrete design settings"]
["STEP [m]","WIDTH MIN [m]","WIDTH MAX [m]","LENGTH MIN [m]","LENGTH MAX [m]","HEIGHT MIN  [m]","HEIGHT MAX [m]","Lx = Ly"]
[0.5,1,2,0.5,4,0.5,1.5,false]
[]
[]
["General"]
["Limit utilization"]
[0.7]

{"sheet":"Enums","index":7,"n_rows":23,"n_cols":21,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
["Annex","Concrete","Reinforcement","Exposure","Reliability","Consequence","Foundation Distribution","Fabrication","Inspection Level","Life Category","Design Approach","Geotechnical Category","Soil Punching Type","Direction","Combination","Zone","Diameter","Soil","Foundation type","Soil calculation","Boolean"]
["ANNEX_COMMON","C12/15","B500","EXPOSURE_CLASS_X0","RELIABILITY_CLASS_1","CONSEQUENCE_CLASS_1","FOUNDATION_DISTRIBUTION_ELASTIC","FABRICATION_IN_SITU","INSPECTION_LEVEL_RELAXED","LIFE_CATEGORY_L20","DESIGN_APPROACH_1","GEOTECHNICAL_CATEGORY_1","SOIL_PUNCHING_TYPE_WIDTH_1_2","X","CHARACTERISTIC","BOTTOM",6,"Drained","Point","Simple",true]
["ANNEX_DENMARK","C16/20","N","EXPOSURE_CLASS_XC1","RELIABILITY_CLASS_2","CONSEQUENCE_CLASS_2","FOUNDATION_DISTRIBUTION_PLASTIC","FABRICATION_PREFAB","INSPECTION_LEVEL_NORMAL","LIFE_CATEGORY_L50","DESIGN_APPROACH_2","GEOTECHNICAL_CATEGORY_2","SOIL_PUNCHING_TYPE_1_2","Y","FREQUENT","TOP",8,"Undrained","Line","Complex",false]
["ANNEX_SWEDEN","C20/25","K","EXPOSURE_CLASS_XC2","RELIABILITY_CLASS_3","CONSEQUENCE_CLASS_3",null,null,"INSPECTION_LEVEL_TIGHTENED","LIFE_CATEGORY_L100","DESIGN_APPROACH_3","GEOTECHNICAL_CATEGORY_3","SOIL_PUNCHING_TYPE_1_3",null,"QUASI_PERMANENT",null,10,"Rock"]
["ANNEX_NORWAY","C25/30","Y","EXPOSURE_CLASS_XC3",null,null,null,null,null,null,null,null,"SOIL_PUNCHING_TYPE_1_4",null,"ULTIMATE",null,12,"Combined"]
["ANNEX_FINLAND","C28/35","Z","EXPOSURE_CLASS_XC4",null,null,null,null,null,null,null,null,null,null,"ACCIDENTAL",null,14]
["ANNEX_GREAT_BRITAIN","C30/37","R","EXPOSURE_CLASS_XD1",null,null,null,null,null,null,null,null,null,null,"SEISMIC",null,16]
[null,"C32/40","Ss260","EXPOSURE_CLASS_XD2",null,null,null,null,null,null,null,null,null,null,null,null,20]
[null,"C35/45","B500B","EXPOSURE_CLASS_XD3",null,null,null,null,null,null,null,null,null,null,null,null,25]
[null,"C40/50","Ks600","EXPOSURE_CLASS_XS1",null,null,null,null,null,null,null,null,null,null,null,null,32]
[null,"C45/55","Ps500","EXPOSURE_CLASS_XS2",null,null,null,null,null,null,null,null,null,null,null,null,40]
[null,"C50/60","G250","EXPOSURE_CLASS_XS3"]
[null,"C54/65","B500A","EXPOSURE_CLASS_XA1"]
[null,"C55/67","B500B","EXPOSURE_CLASS_XA2"]
[null,"C58/70","B500C","EXPOSURE_CLASS_XA3"]
[null,"C60/75","S235JRG2","EXPOSURE_CLASS_XF1"]
[null,"C70/85","A500HW","EXPOSURE_CLASS_XF2"]
[null,"C80/95","A700HW","EXPOSURE_CLASS_XF3"]
[null,"C90/105","B500K","EXPOSURE_CLASS_XF4"]
[null,null,"B600KX"]
[null,null,"B700K"]
[null,null,"_250"]
[null,null,"_420"]